
[image: LOGO 50x50mm PNG_画板 1]              Professional Audio/Visual Over Fiber Solution Manufacturer

4K Single LC Fiber Extender with Pigtail: USB-C to USB-C
 
[bookmark: _GoBack]OCTOPUS-CC-P01
OCTOPUS-CC-P01 is a full 4k UHD video fiber extender, which resolution is up to 4096*2016@ 60Hz 4:4:4 (DSC2:1). This USB-C fiber extender delivers a maximum bandwidth of 18Gbps. It fully supports DP Alt Mode and is compatible with both single-mode (SMF) and multi-mode (MMF) fibers. The transmission distance is up to 300M over MMF and 20KM over SMF.

The extender pair is using CWDM technology, there are 2 wavelength lasers in the extender pair, 1270nm and 1330nm.
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Optical
Optical source: CWDM DFB Laser
Fiber: 1 core LC, Single Mode or Multi Mode
Distance:  MM:300M  SM:20KM
                                                                         
    
                              
Package
TX x 1
RX x 1
5V/1A power adapter x 2
USB-A to USB-C cable x2
)Features
· Support 18Gbps video bandwidth.
· Video resolution up to 3840*2160 50/60HZ(YUV 4:4:4).
· Support DP Alt Mode and compliant with DP 1.2.
· Support LPCM 7.1CH, AES67, DSD, Dolby 5.1, Dolby Atmos, DTS：X Audio.
· EDID management through USB Type-C(female), support EDID pass-through and auto-adaptation. Built-in fixed list of commonly used EDIDs, allowing reading, displaying, and saving the EDID of the display end, and also support direct writing of .bin files.
· Transmission distance up to 300 meters over OM3 Multi-mode fiber, or 20KM over single-mode fiber.
· Low EMI.
· Compact size and detachable structure, easy and flexible for installation.
· Support mixed matching and interconnection with other interfaces (HDMI, DVI, DP) in the same product series.
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Specification
	 
	Transmitter
	Receiver

	Compliance
	DP1.2

	HDCP
	-

	Video Bandwidth
	18Gbps

	Distance
	Single-mode fiber: 20KM
Multi-mode fiber: 300M

	Supporting Resolution 
	4Kx2K@60HZ(4:4:4 8bit)

	Connector/Fiber
	USB-C (male)/ LC
	LC/USB-C(male)

	CWDM filter
	Integrated 1270nm/1310nm filter

	Power Supply
	5V/1A
	5V/1A

	Power Consumption
	3W
	2W

	Color
	Black
	Black

	Dimension(LxWxH)
	Pigtail: 190MM

	
	Model: 64x35x12.3MM
	Model: 64x35x12.3MM

	
	Package:250x180x37MM

	Weight
	Model: 85 g
	Model: 85 g

	
	Package：450 g

	Environment
	[bookmark: OLE_LINK2]Operating Temperature Range:  -10°C~60°C
Storage Temperature Range: -40°C~85°C

	Relative Humidity
	20-90% RH (no condensation)
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